B03C Group 15

Members:

Nimesha Witharana, nwit968

Yonghui Tao, ytao624

Execution Description:

Connect the following pins on the STK500 Board:

PB0 => LED0

PB1 => LED1

PB2 => LED2

PB4 => LED4

PB5 => LED3

PD0 => SW3

PD1 => SW4

PD2 => SW7

PD3 => SW0

PD5=> SW5

PD6=> SW6

Potentiometer to VTG, GND, PC0

Oscilloscope probe for PWM => PB3

Press SW4 to toggle for task 4 PWM

Press SW3 to toggle for task 3 PWM